M9703A Plott Tool1

1. First check wheterh you want log scale and/or background subtraction  
2. Select the file to plot  
3. Edit fields for Y-plotrange and Y-plotrange





Fig. 1: Spectral overview expressed in dB including background subtraction.

  
Fig. 2: Zoom into military satellite downlinks. A Y-factor of 10 dB proofs that the system is o.k.